Please see below responses to clarifications raised to date and an amendment to the pricing sheet relating to SE 1.2 and SE 1.3. Please use Pricing sheet R2.

SE 1.2 should be: 1

SE 1.3 should be: 4

Questions:

* There is mention of Orchestra pit control in the responsibility matrix. Can I just confirm there is no orchestra pit to be installed by bidders?

 I can confirm there is no Orchestra pit

* The pricing schedule lists 6x4 deck. Can I just check is this supposed to be 8x4 deck please?

No, it is for 6x4 deck for them to be stored on end in the seating store

Please also note the maximum depth of the Rosta 100mm

* The cinema specification is for a 7m wide screen. I’ve been advised a 6.5m wide screen is much cheaper. Will this be accepted as an option?

It can be considered as an option please price for both 7m and 6.5m

* The responsibility matrix suggests the GE will supply data wiring for the stage lighting system. Can I just check this will be the case?

YES

Can I clarify the following on stage engineering please…

* The house tabs curtain track and border will be suspended from the pros frame and that this is being custom manufactured by others?

No, it is part of the tender the :  SE 1.8 on the pricing sheet / 3.3.2 House Curtain Header frame and track in Performance Spec

* The requirement is for 8 manual/drill winches on stage, with an option for these to be electric, all with a SWL of 250kg except the U/S hoist which is to be 500kg, or is there a need for other bars to be 500kg too?

The 2 FOH bars should be electric

The first 3 bars OH should be an option for electric full list below:

FOH 1 electric 250kg

FOH 2 electric 250kg

OH 1 electric 500kg

OH 2 electric 250kg

OH 3  electric 250kg

OH 4 fixed 250kg

OH 5 500kg Manual/Drill

OH 6. 250kg Manual/Drill

OH 7 500kg Manual/Drill

OH 8 500kg Manual/Drill

OH 9 500kg Manual/Drill

* The FOH bars will be manual/drill hoists but you’d like an option for these to be electric?

These should be Electric 250kg

* The legs, borders and drape track will be suspended from the ladder bars/hoists and a single fixed bar? Or is this to be fixed and not part of the hoist system?

To be suspended from the Ladder bars and or single fixed bar